{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Mitat","Yksikkö","","Korkeus","mm","870","870"]
["","","","Leveys","mm","1,100","1,100"]
["","","","Syvyys","mm","460","460"]
["Paino","Yksikkö","","","kg","101","101"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","85.0","85.0"]
["","","Jäähdytys","Suuri","m³/min","85","85"]
["Toimintalämpötila-alue","Jäähdytys","","Min.","°CDB","10","10"]
["","","","Maks.","°CDB","43","43"]
["","Kuuma käyttövesi","","Min.","°CDB","-25","-25"]
["","","","Maks.","°CDB","25 (1), 35 (1)","25 (1), 35 (1)"]
["Äänen tehotaso","Lämmitys","","Nimell.","dBA","62.0 (2)","62.0 (2)"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","48.0 (2)","48.0 (2)"]
["Kylmäaine","Tyyppi","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Täytösmäärä","","","tCO2Eq","2.57","2.57"]
["","Täytösmäärä","","","kg","3.8","3.8"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.5","9.5"]
["","Kaasu","","Ulkohalkaisija","mm","15.9","15.9"]
["Putkistoliitännät","Tyhjennys","","Ulkohalkaisija","mm","26","26"]
["","Korkeusero","IU - OU","Maks.","m","30.0","30.0"]
["Putkiliitännät","Lämmöneristys","","","","Sekä neste- että kaasuputket","Sekä neste- että kaasuputket"]
["Virransyöttö","Nimi","","","","W1","W1"]
["","Vaihe","","","","3~","3~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","400","400"]
["Virta","Suositeltu sulakekoko","","","A","16","16"]
["Huomautukset","","","","","(1) - Lisätietoja on toimintalämpötila-alueen piirroksessa","(1) - Lisätietoja on toimintalämpötila-alueen piirroksessa"]
["","","","","","(2) - Mitattu lämmitysjärjestelmän 10 kPa painehäviöllä käyttöolosuhteissa, joissa lähtevään veden lämpötila on 47 - 55 °C huoneessa, jonka lämpötila on 20 °C. DB/WB 7°C/6°.","(2) - Mitattu lämmitysjärjestelmän 10 kPa painehäviöllä käyttöolosuhteissa, joissa lähtevään veden lämpötila on 47 - 55 °C huoneessa, jonka lämpötila on 20 °C. DB/WB 7°C/6°."]