{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / ARXM-A"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / ARXM71A5V1B"]
["Jäähdytysteho","Nimell.","","kW","6.8"]
["","Maks.","","kW","6.95"]
["Lämmitysteho","Nimell.","","kW","7.5"]
["","Maks.","","kW","7.59"]
["Nimellinen tehokkuus","EER","","","3.4"]
["","COP","","","3.19"]
["","Vuotuinen energiankulutus","","kWh","1000"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","D"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","6.8"]
["","SEER","","","5.77"]
["","Vuotuinen energiankulutus","","kWh/a","412"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A"]
["","Teho","Pdesign","kW","4.5"]
["","SCOP/A","","","3.81"]
["","Pdh Lämmitysteho -10°:ssa","","kW","4.5"]
["","Vuotuinen energiankulutus","","kWh/a","1652"]
["Huomautukset","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista"]