{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen"]
["","Materiaali","","","","Hartsi","Hartsi"]
["Mitat","Yksikkö","","Korkeus","mm","290","340"]
["","","","Leveys","mm","1050","1200"]
["","","","Syvyys","mm","269","262"]
["Paino","Yksikkö","","","kg","14","18"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","16.2","23"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","13.4","21.1"]
["","","","Pieni","m³/min","12.1","18.7"]
["","","Lämmitys","Suuri","m³/min","16.9","23"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","14.2","20.9"]
["","","Lämmitys","Pieni","m³/min","12.7","18.7"]
["Äänen tehotaso","Jäähdytys","","","dBA","61","65"]
["","Lämmitys","","","dBA","61","65"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","45","49"]
["","","","Keski","dBA","42","45"]
["","","","Pieni","dBA","40","41"]
["","Lämmitys","","Suuri","dBA","45","49"]
["","","","Keski","dBA","42","45"]
["","","","Pieni","dBA","40","41"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.9","15.9"]
["","Kondenssi","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]
["Vakiovarusteet","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Huomautukset","","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["Vakiovarusteet","Screw cover","","","","","3"]