{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Äänenpaineen taso","Lämmitys","Suuri","dBA","45","49"]
["","","Nimell.","dBA","42","45"]
["","","Keski","dBA","42","45"]
["","","Pieni","dBA","40","41"]
["","Jäähdytys","Medium","dBA","42","45"]
["","","Pieni","dBA","40","41"]
["","","Suuri","dBA","45","49"]
["","","Nimell.","dBA","42","45"]
["Jäähdytysteho","Kokonaisteho","Nimell.","kW","0.051","0.061"]
["Putkistoliitännät","Neste","Ulkohalkaisija","mm","9.52","9.52"]
["","Kaasu","Ulkohalkaisija","mm","15.9","15.9"]
["","Tyhjennys","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Äänen tehotaso","Jäähdytys","","dBA","61","65"]
["","Lämmitys","","dBA","61","65"]
["Mitat","Yksikkö","Leveys","mm","1,050","1,200"]
["","","Syvyys","mm","238","240"]
["","","Korkeus","mm","290","340"]
["Kotelo","Materiaali","","","Hartsi","Hartsi"]
["","Colour","","","Raikas valkoinen","Raikas valkoinen"]
["Paino","Yksikkö","","kg","13","17"]
["Lämmitysteho","Yhteisteho","Nim.","kW","0.068","0.061"]
["Power supply","Vaihe","","","1~","1~"]
["","Taajuus","","Hz","50","50"]
["","Jännite","","V","220-240","220-240"]