{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A9"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RXM35A5V1B9","FBA50A2VEB9 / RXM50A5V1B9"]
["Jäähdytysteho","Nimell.","","kW","3.4","5"]
["Lämmitysteho","Nimell.","","kW","4","5.5"]
["Nimellinen tehokkuus","EER","","","4.02","3.55"]
["","COP","","","4.02","3.83"]
["","Vuotuinen energiankulutus","","kWh","423","704"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","A","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++","A++"]
["","Teho","Pdesign","kW","3.4","5"]
["","SEER","","","6.3","6.27"]
["","Vuotuinen energiankulutus","","kWh/a","189","279"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+","A+"]
["","Teho","Pdesign","kW","2.9","4.4"]
["","SCOP/A","","","4.17","4.06"]
["","Pdh Lämmitysteho -10°:ssa","","kW","2.32","3.73"]
["","Vuotuinen energiankulutus","","kWh/a","973","1517"]
["Huomautukset","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(4) - Katso sähköiset tiedot eri piirustuksista"]