{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZASG-MY"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZASG100MUY","FBA125A2VEB / RZASG125MUY"]
["Jäähdytysteho","Nimell.","","kW","9.5","12.1 (1)"]
["Lämmitysteho","Nimell.","","kW","10.8 (2)","13.5 (2)"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A"]
["","Teho","Pdesign","kW","9.5","12.1"]
["","SEER","","","5.31","5.49"]
["","Vuotuinen energiankulutus","","kWh/a","626","1322"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A"]
["","Teho","Pdesign","kW","6","6"]
["","SCOP/A","","","3.8","3.63"]
["","Vuotuinen energiankulutus","","kWh/a","2211","2314"]
["Huomautukset","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]