{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","37.0","37.0","31.0","31.0"]
["","","","Keski","dBA","34.0","34.0","28.0","28.0"]
["","","","Pieni","dBA","29.0","29.0","25.0","25.0"]
["","Jäähdytys","","Medium","dBA","32.0","32.0","28.0","28.0"]
["","","","Pieni","dBA","29.0","29.0","25.0","25.0"]
["","","","Suuri","dBA","35.0","35.0","30.0","30.0"]
["Vakiovarusteet","Käyttöopas","","","","1","1","1","1"]
["","Asennusohje","","","","1","1","1","1"]
["","Tyhjennysletku","","","","1","1","1","1"]
["","Tyhjennysletkun metallikiristin","","","","1","1","1","1"]
["","Koukkukiinnikkeen aluslevy","","","","8","8","8","8"]
["","Ruuvit","","","","40","40","40","40"]
["","Asennuseriste","","","","2","2","2","2"]
["","Tiivistysläpät","","","","5","5","5","5"]
["","Siteet","","","","4","4","4","4"]
["Ohjausjärjestelmät","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Piping connections","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","9.52"]
["","Gas","","Ulkohalkaisija","mm","9.52","12.70","12.70","15.90"]
["","Tyhjennys","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Äänen tehotaso","Jäähdytys","","","dBA","60","60","56","56"]
["Mitat","Yksikkö","","Leveys","mm","700","700","1,000","1,000"]
["","","","Syvyys","mm","800","800","800","800"]
["","","","Korkeus","mm","245","245","245","245"]
["Kotelo","Materiaali","","","","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy"]
["","Colour","","","","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)","Maalaamaton (galvanoitu)"]
["Paino","Yksikkö","","","kg","28.0","28.0","35.0","35.0"]
["Puhallin","Ulkoinen staattinen paine","","Suuri","Pa","150","150","150","150"]
["","","","Nim.","Pa","30","30","30","30"]
["","Ilmamäärä","Lämmitys","Suuri","m³/min","15.0","15.0","18.0","18.0"]
["","","","Pieni","m³/min","10.5","10.5","12.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0","15.0"]
["","","Cooling","Pieni","m³/min","10.5","10.5","12.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0","15.0"]
["","","","Suuri","m³/min","15.0","15.0","18.0","18.0"]
["Nostokorkeus","mm","","","","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Taajuus","","","Hz","50/60","50/60","50/60","50/60"]
["","Jännite","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Huomautukset","","","","","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon."]
["","","","","","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista"]