{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXS35L3V1B"]
["Jäähdytysteho","Nimell.","","kW","3.40"]
["Lämmitysteho","Nimell.","","kW","4.20"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","455"]
["","COP","","","3.50"]
["","EER","","","3.74"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","B"]
["Putkiliitännät","Tyhjennys","Ulkohalkaisija","mm","VP25 (ulkohalk.32, sisähalk. 25)"]
["","Kaasu","Ulkohalkaisija","mm","9.50"]
["","Neste","Ulkohalkaisija","mm","6.35"]
["Huomautukset","","","","(1) - Normaali toiminta: +22°C / + 32°C"]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista"]