{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZAG-B"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RZAG35B5V1B","FCAG50BVEB / RZAG35B5V1B","FCAG60BVEB / RZAG50B5V1B","FCAG50BVEB / RZAG50B5V1B","FCAG60BVEB / RZAG60B5V1B","FCAG71BVEB / RZAG60B5V1B"]
["Jäähdytysteho","Min.","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Nimell.","","kW","3.5","3.5","5","5","6","6"]
["","Maks.","","kW","4.5","4.5","6","6","6.5","6.5"]
["Lämmitysteho","Min.","","kW","1.4","1.4","1.5","1.5","1.6","1.6"]
["","Nimell.","","kW","4","4","5.8","5.8","7","7"]
["","Maks.","","kW","5","5","6","6","7.5","7.5"]
["Nimellinen tehokkuus","EER","","","4.4","4.57","3.98","3.9","3.4","3.79"]
["","COP","","","4.3","4.41","3.75","3.71","3.4","3.53"]
["","Vuotuinen energiankulutus","","kWh","398","383","628","641","882","792"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A","A","A","A","A"]
["","","Lämmitys","","A","A","A","A","C","B"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++","A++","A++","A++","A++","A++"]
["","Teho","Pdesign","kW","3.5","3.5","5","5","6","6"]
["","SEER","","","7.3","7.4","6.93","6.8","6.6","6.82"]
["","Vuotuinen energiankulutus","","kWh/a","168","166","252","257","318","308"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+","A+","A+","A+","A+","A+"]
["","Teho","Pdesign","kW","3.3","3.3","4.3","4.3","4.6","4.6"]
["","SCOP/A","","","4.3","4.41","4.35","4.3","4.25","4.39"]
["","Pdh Lämmitysteho -10°:ssa","","kW","2.91","2.91","3.73","3.68","3.96","4"]
["","Vuotuinen energiankulutus","","kWh/a","1074","1048","1384","1398","1515","1467"]