{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Jäähdytysteho","Nimell.","","kW","","","","","","","6.80","6.80","13.40"]
["Tilan jäähdytys","SEER","","","","","","","","","6.91","6.91","6.75"]
["","ηs,c","","%","","","","","","","","","266.88"]
["","Vuotuinen energiankulutus","","kWh/a","","","","","","","345","345","1,191"]
["","Teho","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Energiatehokkuusluokka","","","","","","","","","A++","A++"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Energiatehokkuusluokka","","","","","","","","","A+","A+"]
["","Vuotuinen energiankulutus","","kWh/a","","","","","","","2,344","2,344","3,766"]
["","ηs,h","","%","","","","","","","","","172.10"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","","","","","","","831"]
["","EER","","","","","","","","","4.09","4.09","3.18"]
["","COP","","","","","","","","","4.80","","4.12"]
["","Energiamerkintädirektiivi","Jäähdytys","","","","","","","","A"]
["","","Lämmitys","","","","","","","","A"]
["Lämmitysteho","Nimell.","","kW","","","","","","","7.50","","15.50"]
["Huomautukset","","","","","","","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","","","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","","","","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","","","","","","(4) - Katso sähköiset tiedot eri piirustuksista","","(4) - Katso sähköiset tiedot eri piirustuksista"]
["Energiatehokkuusalue","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]