{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-K"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35K2V1B","FCQG50FVEB / RXS50K2V1B"]
["Jäähdytysteho","Nimell.","","kW","3.40","5.00"]
["Piping connections","Neste","Ulkohalkaisija","mm","6.35","6.35"]
["","Kaasu","Ulkohalkaisija","mm","9.5","12.7"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","475","705"]
["","EER","","","3.58","3.55"]
["","COP","","","3.41","3.70"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","B","A"]
["Lämmitysteho","Nimell.","","kW","4.20","6.00"]
["Huomautukset","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]