{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":117,"n_cols":9,"rows_kept":117,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","44","45","45"]
["","","","Nimell.","dBA","","39","40","41"]
["","","","Pieni","dBA","","33","35","37"]
["","Jäähdytys","","Pieni","dBA","","33","35","37"]
["","","","Suuri","dBA","","44","45","45"]
["","","","Nimell.","dBA","","39","40","41"]
["Vakiovarusteet","Käyttöopas","","","","","Käyttöopas","Käyttöopas","Käyttöopas"]
["","Asennusohje","","","","","Asennusohje","Asennusohje","Asennusohje"]
["","Tyhjennysletku","","","","","Tyhjennysletku","Tyhjennysletku","Tyhjennysletku"]
["","Tyhjennysletkun kiristin","","","","","Tyhjennysletkun kiristin","Tyhjennysletkun kiristin","Tyhjennysletkun kiristin"]
["","Koukkukiinnikkeen aluslevy","","","","","Koukkukiinnikkeen aluslevy","Koukkukiinnikkeen aluslevy","Koukkukiinnikkeen aluslevy"]
["","Ruuvit","","","","","Ruuvit","Ruuvit","Ruuvit"]
["","Asennusopas","","","","","Asennusopas","Asennusopas","Asennusopas"]
["","Asennuseriste","","","","","2","2","2"]
["","Tiivistysläpät","","","","","4","4","4"]
["","Tyhjennyksen tiivistysläppä","","","","","Tyhjennyksen tiivistysläppä","Tyhjennyksen tiivistysläppä","Tyhjennyksen tiivistysläppä"]
["","Siteet","","","","","Siteet","Siteet","Siteet"]
["Control systems","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Putkikoot","Neste","","Ulkohalkaisija","mm","","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","","15.9","15.9","15.9"]
["","Tyhjennys","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Säleikkö 4","Mitat","","Syvyys","mm","","50","50","50"]
["","","","Leveys","mm","","950","950","950"]
["","","","Korkeus","mm","","950","950","950"]
["","Malli","","","","","BYCQ140D7W1 - valkoinen harmaalla säleiköllä","BYCQ140D7W1 - valkoinen harmaalla säleiköllä","BYCQ140D7W1 - valkoinen harmaalla säleiköllä"]
["","Väri","","","","","Puhdas valkoinen (RAL 9010)","Puhdas valkoinen (RAL 9010)","Puhdas valkoinen (RAL 9010)"]
["","Paino","","","kg","","5.4","5.4","5.4"]
["Sound power level","Jäähdytys","","","dBA","","61","61","61"]
["","Lämmitys","","","dBA","","61","61","61"]
["Mitat","Unit","","Width","mm","","840","840","840"]
["","","","Depth","mm","","840","840","840"]
["","","","Height","mm","","288","288","288"]
["Casing","Material","","","","","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy"]
["Paino","Unit","","","kg","","26","26","26"]
["Säleikkö","Paino","","","kg","","10.3","10.3","10.3"]
["","Model","","","","","BYCQ140D7GFW1 - automaattisesti puhdistuva paneeli hienolla verkkosuodattimella","BYCQ140D7GFW1 - automaattisesti puhdistuva paneeli hienolla verkkosuodattimella","BYCQ140D7GFW1 - automaattisesti puhdistuva paneeli hienolla verkkosuodattimella"]
["","Mitat","","Korkeus","mm","","130","130","130"]
["","","","Syvyys","mm","","950","950","950"]
["","","","Leveys","mm","","950","950","950"]
["","Väri","","","","","Valkoinen (RAL 9010)","Valkoinen (RAL 9010)","Valkoinen (RAL 9010)"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Taajuus","","","Hz","","50","50","50"]
["","Name","","","","","VE","VE","VE"]
["","Jännite","","","V","","220-240","220-240","220-240"]
["Huomautukset","","","","","","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(1) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon."]
["","","","","","","(2) - Mallissa BYCQ140D7W1W on valkoiset eristeet. Huomaa, että lian muodostuminen näkyy valkoisilla pinnoilla paremmin. Siten BYCQ140D7W1W-koristepaneelia ei suositella käytettäväksi likaisissa olosuhteissa.","(2) - Mallissa BYCQ140D7W1W on valkoiset eristeet. Huomaa, että lian muodostuminen näkyy valkoisilla pinnoilla paremmin. Siten BYCQ140D7W1W-koristepaneelia ei suositella käytettäväksi likaisissa olosuhteissa.","(2) - Mallissa BYCQ140D7W1W on valkoiset eristeet. Huomaa, että lian muodostuminen näkyy valkoisilla pinnoilla paremmin. Siten BYCQ140D7W1W-koristepaneelia ei suositella käytettäväksi likaisissa olosuhteissa."]
["","","","","","","(3) - BYCQ140D7W1: puhtaanvalkoinen vakiosäleiköllä ja harmailla puhallusilmanohjaimilla; BYCQ140D7W1W: puhtaanvalkoinen vakiosäleiköllä ja valkoisilla puhallusilmanohjaimilla; BYCQ140D7GW1: puhtaanvalkoinen automaattisesti puhdistuvalla säleiköllä.","(3) - BYCQ140D7W1: puhtaanvalkoinen vakiosäleiköllä ja harmailla puhallusilmanohjaimilla; BYCQ140D7W1W: puhtaanvalkoinen vakiosäleiköllä ja valkoisilla puhallusilmanohjaimilla; BYCQ140D7GW1: puhtaanvalkoinen automaattisesti puhdistuvalla säleiköllä.","(3) - BYCQ140D7W1: puhtaanvalkoinen vakiosäleiköllä ja harmailla puhallusilmanohjaimilla; BYCQ140D7W1W: puhtaanvalkoinen vakiosäleiköllä ja valkoisilla puhallusilmanohjaimilla; BYCQ140D7GW1: puhtaanvalkoinen automaattisesti puhdistuvalla säleiköllä."]
["Kotelo","Materiaali","","","","Galvanoitu teräslevy"]
["Mitat","Yksikkö","","Korkeus","mm","288"]
["","","","Leveys","mm","840"]
["","","","Syvyys","mm","840"]
["Paino","Yksikkö","","","kg","25"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","21.2"]
["","","","Nimell.","m³/min","16.7"]
["","","","Pieni","m³/min","12.2"]
["","","Lämmitys","Suuri","m³/min","21.2"]
["","","","Nimell.","m³/min","16.7"]
["","","","Pieni","m³/min","12.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","53"]
["","Lämmitys","","","dBA","53"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","36"]
["","","","Nimell.","dBA","33"]
["","","","Pieni","dBA","29"]
["","Lämmitys","","Suuri","dBA","36"]
["","","","Nimell.","dBA","33"]
["","","","Pieni","dBA","29"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.9"]
["","Kondenssi","","","","VP25 (I.D. 25/O.D. 32)"]
["Säleikkö","Malli","","","","BYCQ140D7GFW1 - automaattisesti puhdistuva paneeli hienolla verkkosuodattimella"]
["","Väri","","","","Valkoinen (RAL 9010)"]
["","Mitat","","Korkeus","mm","130"]
["","","","Leveys","mm","950"]
["","","","Syvyys","mm","950"]
["","Paino","","","kg","10.3"]
["Säleikkö 2","Malli","","","","BYCQ140D7GW1 - Automaattisesti puhdistuva säleikkö"]
["","Väri","","","","Valkoinen (RAL 9010)"]
["","Mitat","","Korkeus","mm","130"]
["","","","Leveys","mm","950"]
["","","","Syvyys","mm","950"]
["","Paino","","","kg","10.3"]
["Säleikkö 3","Malli","","","","BYCQ140D7W1W - Kokovalkoinen"]
["","Väri","","","","Valkoinen (RAL 9010)"]
["","Mitat","","Korkeus","mm","50"]
["","","","Leveys","mm","950"]
["","","","Syvyys","mm","950"]
["","Paino","","","kg","5.4"]
["Säleikkö 4","Malli","","","","BYCQ140D7W1 - Valkoinen, harmaat ilmanohjaimet"]
["","Väri","","","","Valkoinen (RAL 9010)"]
["","Mitat","","Säleikkö 4-=-Mitat-=-Korkeus-=-mm","mm","950"]
["","","","Leveys","mm","950"]
["","","","Syvyys","mm","50"]
["","Paino","","","kg","5.4"]
["Control systems","Infrared remote control","","","","BRC7FA532F"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","BRC1D52, BRC1E52A/B"]
["Vakiovarusteet","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Virransyöttö","Nimi","","","","VE"]
["","Vaihe","","","","1~"]
["Syöttöjännite","Syöttöjännite-=-Taajuus","","Taajuus","","50"]
["","Syöttöjännite-=-Jännite","","Jännite","","220-240"]