{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZQSG125L9V1B"]
["Jäähdytysteho","Nimell.","","kW","12.00"]
["Tilan jäähdytys","SEER","","","5.20"]
["","Vuotuinen energiankulutus","","kWh/a","808"]
["","Teho","Pdesign","kW","12.00"]
["","Energiatehokkuusluokka","","","A"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","7.60"]
["","SCOP/A","","","3.90"]
["","Energiatehokkuusluokka","","","A"]
["","Vuotuinen energiankulutus","","kWh/a","2,729"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","1,942"]
["","EER","","","3.09"]
["","COP","","","3.51"]
["","Energiamerkintädirektiivi","Jäähdytys","","B"]
["","","Lämmitys","","B"]
["Lämmitysteho","Nimell.","","kW","13.50"]
["Huomautukset","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista"]