{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Jäähdytysteho","Yhteisteho","","Nimell.","kW","12.10","19.00","22.00"]
["Lämmitysteho","Yhteisteho","","Nim.","kW","13.50","22.4","24.0"]
["Casing","Väri","","","","Maalaamaton","Maalaamaton","Maalaamaton"]
["","Material","","","","Galvanoitu teräs","Galvanoitu teräslevy","Galvanoitu teräslevy"]
["Mitat","Yksikkö","","Korkeus","mm","300","470","470"]
["","","","Leveys","mm","1,400","1,490","1,490"]
["","","","Syvyys","mm","700","1,100","1,100"]
["Paino","Yksikkö","","","kg","45","104","115"]
["Tarvittava alakaton asennustila >","mm","","","","350"]
["Fan","Ilmamäärä","Jäähdytys","Suuri","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50","56"]
["","","","Pieni","m³/min","28.0","36.0","43.0"]
["","","Lämmitys","Suuri","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50.0","56.0"]
["","","","Pieni","m³/min","28.0","36.0","43.0"]
["","Ulkoinen staattinen paine","","Suuri","Pa","200","250","250"]
["","","","Nimell.","Pa","50","62","62"]
["Äänen tehotaso","Jäähdytys","","","dBA","66","69.0","71.0"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Pieni","dBA","33","36.0","37.0"]
["","Lämmitys","","Suuri","dBA","40","43.0","44.0"]
["","","","Keski","dBA","","39.0","40.0"]
["","","","Pieni","dBA","33","36.0","37.0"]
["Piping connections","Liquid","","Ulkohalkaisija","mm","9.52","9.52","9.52"]
["","Gas","","Ulkohalkaisija","mm","15.90","19.1","22.2"]
["","Tyhjennys","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Nostokorkeus","mm","","","","625"]
["Säleikkö","Model","","","","BYBS125DJW1"]
["","Väri","","","","Valkoinen (10Y9/0,5)"]
["","Mitat","","Korkeus","mm","55"]
["","","","Leveys","mm","1,500"]
["","","","Syvyys","mm","500"]
["","Paino","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Vakiovarusteet","Ruuvit","","","","16","2","2"]
["","Aluslevy","","","","8","12","12"]
["","Letkun nauha","","","","1"]
["","Tyhjennysletku","","","","1"]
["","Yleiset varotoimet","","","","1","1","1"]
["","Asennus- ja käyttöohje","","","","1","1","1"]
["","Yleinen virransyöttöjohto","","","","2"]
["","Tiivistysmateriaali (tyhjennysletku)","","","","1"]
["","Tiivistysmateriaali","","","","2"]
["","Lämpöeristeputki (neste)","","","","1"]
["","Lämpöeristeputki (kaasu)","","","","1"]
["Power supply","Name","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Taajuus","","","Hz","50/60","50/60","50/60"]
["","Jännite","","","V","220-240/220","220-240/220","220-240/220"]
["Huomautukset","","","","","(1) - Katso sähköiset tiedot eri piirustuksista"]
["Vakiovarusteet","Käyttöopas","","","","","1","1"]
["","Asennusohje","","","","","1","1"]
["","Kaasun liitäntäputki","","","","","1","1"]
["","Johtimen kiinnitysmateriaali","","","","","1","1"]
["","Jousialuslevy","","","","","2","2"]
["","Ruuvi + aluslevy","","","","","45","45"]
["","Kuusiokantapultti ja aluslevy","","","","","49","49"]
["","Kuusiokantapultti","","","","","2","2"]
["","Suora aluslevy","","","","","8","8"]