{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","35.0","35.0"]
["","","","Pieni","dBA","29.0","29.0"]
["","Jäähdytys","","Pieni","dBA","28.0","28.0"]
["","","","Suuri","dBA","35.0","35.0"]
["Vakiovarusteet","Asennus- ja käyttöohje","","","","1","1"]
["","Imuilmansuodatin","","","","1","1"]
["Control systems","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.52"]
["","Kondenssi","","","","27.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","55","55"]
["","Lämmitys","","","dBA","55","55"]
["Mitat","Yksikkö","","Leveys","mm","652","652"]
["","","","Syvyys","mm","502","502"]
["","","","Korkeus","mm","230","230"]
["Kotelo","Materiaali","","","","Sinkkipinnoitettu niukkahiiliteräs","Sinkkipinnoitettu niukkahiiliteräs"]
["Paino","Yksikkö","","","kg","17.0","17.0"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","","6.95"]
["","","","Pieni","m³/min","","5.20"]
["","","Jäähdytys","Pieni","m³/min","","5.20"]
["","","","Suuri","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Taajuus","","","Hz","50","50"]
["","Nimi","","","","V1","V1"]
["","Jännite","","","V","230","230 +/-10%"]
["Huomautukset","","","","","(1) - Ääniarvot mitataan puolikaiuttomassa huoneessa.","(1) - Ääniarvot mitataan puolikaiuttomassa huoneessa."]
["","","","","","(2) - Äänen painetaso on suhteellinen ja määräytyy etäisyyden ja akustiikan mukaan. Lisätietoja on äänitasopiirustuksissa.","(2) - Äänen painetaso on suhteellinen ja määräytyy etäisyyden ja akustiikan mukaan. Lisätietoja on äänitasopiirustuksissa."]
["","","","","","(3) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(3) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon."]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","9.52"]
["","Kondenssi","","","","","27.2"]