{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQG125L9V1B"]
["Jäähdytysteho","Nimell.","","kW","12.0"]
["Tilan jäähdytys","SEER","","","5.81"]
["","Vuotuinen energiankulutus","","kWh/a","723"]
["","Teho","Pdesign","kW","12.00"]
["","Energiatehokkuusluokka","","","A+"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","12.71"]
["","SCOP/A","","","4.21"]
["","Energiatehokkuusluokka","","","A+"]
["","Vuotuinen energiankulutus","","kWh/a","4,227"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","1,600"]
["","EER","","","3.75"]
["","COP","","","3.83"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Lämmitysteho","Nimell.","","kW","13.5"]
["Huomautukset","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]