{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Jäähdytysteho","Min.","","kW","","1.70"]
["","Nimell.","","kW","","6.00"]
["","Maks.","","kW","","6.50"]
["Lämmitysteho","Min.","","kW","","1.70"]
["","Nimell.","","kW","","7.00"]
["","Maks.","","kW","","7.10"]
["Nimellinen tehokkuus","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Annual energy consumption","","kWh","","1,024"]
["","Energiamerkintädirektiivi","Jäähdytys","","","C"]
["","","Lämmitys","","","C"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","A"]
["","Teho","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Vuotuinen energiankulutus","","kWh/a","","378"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","A"]
["","Teho","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Vuotuinen energiankulutus","","kWh/a","","1,693"]
["Huomautukset","","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(2) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","","(3) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","","(4) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Jäähdytysteho","Min.","","kW","1.70"]
["","Nimell.","","kW","5.00"]
["","Maks.","","kW","5.30"]
["Lämmitysteho","Min.","","kW","1.70"]
["","Nimell.","","kW","5.80"]
["","Maks.","","kW","6.00"]
["Nimellinen tehokkuus","EER","","","3.06"]
["","COP","","","3.10"]
["","Vuotuinen energiankulutus","","kWh","816"]
["","Energiamerkintädirektiivi","Jäähdytys","","B"]
["","","Lämmitys","","D"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Vuotuinen energiankulutus","","kWh/a","303"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A"]
["","Teho","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh Lämmitysteho -10°:ssa","","kW","3.55"]
["","Vuotuinen energiankulutus","","kWh/a","1424"]
["Energiatehokkuusalue","","","","A+++ ~ D"]