{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG71M7V1B","FDXM35F3V1B / FDXM35F3V1B / RZAG71M7V1B","FDXM50F3V1B / FDXM50F3V1B / RZAG71M7V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7V1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZAG100M7V1B","FDXM50F3V1B / FDXM50F3V1B / RZAG100M7V1B"]
["Jäähdytysteho","Nimell.","","kW","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Tilan jäähdytys","Vuotuinen energiankulutus","","kWh/a","377","380","334","423","416","379","387"]
["","Teho","Pdesign","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","4.70","4.70","4.70","7.80","7.80","7.80","7.80"]
["","Vuotuinen energiankulutus","","kWh/a","1,537","1,589","1,485","2,540","2,438","2,324","2,421"]
["Lämmitysteho","Nimell.","","kW","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Tilan jäähdytys","SEER","","","6.32","6.27","7.12","7.86","8.00","8.77","8.60"]
["","Energiatehokkuusluokka","","","A++","A++","A++","A++","A++","A+++","A+++"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","SCOP/A","","","4.28","4.14","4.43","4.30","4.48","4.70","4.51"]
["","Energiatehokkuusluokka","","","A+","A+","A+","A+","A+","A++","A+"]
["Huomautukset","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19.0°CWB; ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]