{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.036","0.036","0.060","0.060"]
["","Lämmitys","","Nimell.","kW","0.036","0.036","0.060","0.060"]
["Mitat","Yksikkö","","Korkeus","mm","200","200","200","200"]
["","","","Leveys","mm","750","750","1150","1150"]
["","","","Syvyys","mm","620","620","620","620"]
["Paino","Yksikkö","","","kg","21","21","28","28"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","8.7","8.7","15.8","16.0"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","8.0","8.0","14.6","14.8"]
["","","","Pieni","m³/min","7.3","7.3","13.3","13.5"]
["","","Lämmitys","Suuri","m³/min","8.7","8.7","15.8","16.0"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.0","8.0","14.6","14.8"]
["","","Lämmitys","Pieni","m³/min","7.3","7.3","13.3","13.5"]
["","Ulkoinen staattinen paine","","Nim.","Pa","30","30","40","40"]
["Äänen tehotaso","Jäähdytys","","","dBA","53.0","53.0","55.0","56.0"]
["","Lämmitys","","","dBA","53.0","53.0","55.0","56.0"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","35.0","35.0","38.0","38.0"]
["","","","Keski","dBA","33.0","33.0","35.0","35.0"]
["","","","Pieni","dBA","27.0","27.0","30.0","30.0"]
["","Lämmitys","","Suuri","dBA","35.0","35.0","38.0","38.0"]
["","","","Keski","dBA","33.0","33.0","35.0","35.0"]
["","","","Pieni","dBA","27.0","27.0","30.0","30.0"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50","9.50","12.70","12.70"]
["","Kondenssi","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Vakiovarusteet","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Clamp metal","","","","1","1","1","1"]
["","Clamps","","","","6","6","6","6"]
["","Drain hose","","","","1","1","1","1"]
["","Ilmansuodatin","","","","1","1","1","1"]
["","Insulation for fitting","","","","1","1","1","1"]
["","Screws for duct flanges","","","","1","1","1","1"]
["","Sealing material","","","","2","2","2","2"]
["","Sealing pad","","","","1","1","1","1"]
["","Washer fixing plate","","","","4","4","4","4"]
["Energiatehokkuusalue","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240","220-240"]
["Huomautukset","","","","","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista"]