{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","35.0","35.0","","38.0"]
["","","","Keski","dBA","33.0","33.0","","35.0"]
["","","","Pieni","dBA","27.0","27.0","","30.0"]
["","Jäähdytys","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Pieni","dBA","27.0","27.0","","30.0"]
["","","","Suuri","dBA","35.0","35.0","","38.0"]
["Vakiovarusteet","Asennusohje","","","","1","1","","1"]
["","Käyttöopas","","","","1","1","","1"]
["","Asennuseriste","","","","1","1","","1"]
["","Tiivistysläppä","","","","1","1","","1"]
["","Metalliside","","","","1","1","","1"]
["","Tyhjennysletku","","","","1","1","","1"]
["","Koukkukiinnikkeen aluslevy","","","","8","8","","8"]
["","Tiivistysmateriaali","","","","2","2","","2"]
["","Siteet","","","","6","6","","6"]
["","Kiinnityslevyn aluslevy","","","","4","4","","4"]
["","Putkiliitoslaippojen ruuvit","","","","1","1","","1"]
["","Ilmansuodatin","","","","1","1","","1"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50","9.50","","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.036","0.036","","0.060"]
["","Lämmitys","","Nimell.","kW","0.036","0.036","","0.060"]
["Äänen tehotaso","Jäähdytys","","","dBA","53.0","53.0","","56.0"]
["","Lämmitys","","","dBA","53.0","53.0","","56.0"]
["Mitat","Yksikkö","","Leveys","mm","750","750","","1,150"]
["","","","Syvyys","mm","620","620","","620"]
["","","","Korkeus","mm","200","200","","200"]
["Paino","Yksikkö","","","kg","21","21","","28"]
["Puhallin","Ulkoinen staattinen paine","","Nim.","Pa","30","30","","40"]
["","Ilmamäärä","Lämmitys","Suuri","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Pieni","m³/min","7.3","7.3","","13.5"]
["","","Cooling","Pieni","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Suuri","m³/min","8.7","8.7","","16.0"]
["Power supply","Vaihe","","","","1~","1~","","1~"]
["","Taajuus","","","Hz","50","50","","50"]
["","Jännite","","","V","220-240","220-240","","220-240"]
["Huomautukset","","","","","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista","","(1) - Katso sähköiset tiedot eri piirustuksista"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","","0.060"]
["","Lämmitys","","Nimell.","kW","","","0.060"]
["Mitat","Yksikkö","","Korkeus","mm","","","200"]
["","","","Leveys","mm","","","1150"]
["","","","Syvyys","mm","","","620"]
["Paino","Yksikkö","","","kg","","","28"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","","","15.8"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","","14.6"]
["","","","Pieni","m³/min","","","13.3"]
["","","Lämmitys","Suuri","m³/min","","","15.8"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","","","14.6"]
["","","Lämmitys","Pieni","m³/min","","","13.3"]
["","Ulkoinen staattinen paine","","Nim.","Pa","","","40"]
["Äänen tehotaso","Jäähdytys","","","dBA","","","55.0"]
["","Lämmitys","","","dBA","","","55.0"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","","","38.0"]
["","","","Keski","dBA","","","35.0"]
["","","","Pieni","dBA","","","30.0"]
["","Lämmitys","","Suuri","dBA","","","38.0"]
["","","","Keski","dBA","","","35.0"]
["","","","Pieni","dBA","","","30.0"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","","12.70"]
["","Kondenssi","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Vakiovarusteet","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Ilmansuodatin","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Virransyöttö","Vaihe","","","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","","50"]
["","Jännite","","","V","","","220-240"]