{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Jäähdytysteho","Nimell.","","kW","2.40 (3)"]
["Putkiliitännät","Neste","Ulkohalkaisija","mm","6.35"]
["","Kaasu","Ulkohalkaisija","mm","9.5"]
["","Tyhjennys","Ulkohalkaisija","mm","VP20 (ulkohalk. 26, Sisähalk. 20)"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","345"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","B"]
["Lämmitysteho","Nimell.","","kW","3.20 (4)"]
["Huomautukset","","","","(1) - Energiamerkintä: asteikko ulottuu arvosta A (energiatehokkain) arvoon G (tehottomin)."]
["","","","","(2) - Vuotuinen energiankulutus: perustuu keskimääräiseen 500 käyttötuntiin vuodessa täydellä kuormalla (nimellisolosuhteissa)."]
["","","","","(3) - Jäähdytys: sisälämpötila 27°CDB, 19.0°CWB; ulkolämpötila 35°CDB; putkiston ekvivalenttipituus: 5m; korkeusero: 0m"]
["","","","","(4) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m; korkeusero: 0m"]
["","","","","(5) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]