{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXM25M3V1B9","FFA35A2VEB / RXM35M3V1B9","FFA50A2VEB / RXM50M3V1B9","FFA60A2VEB / RXM60M3V1B9"]
["Jäähdytysteho","Nimell.","","kW","2.50","3.40"]
["Tilan jäähdytys","SEER","","","6.17","6.38"]
["","Vuotuinen energiankulutus","","kWh/a","142","186"]
["","Teho","Pdesign","kW","2.50","3.40"]
["","Energiatehokkuusluokka","","","A++","A++"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Energiatehokkuusluokka","","","A+","A+"]
["","Vuotuinen energiankulutus","","kWh/a","762","1,058"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","273","446"]
["","EER","","","4.57","3.81"]
["","COP","","","3.90","3.50"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","A","B"]
["Lämmitysteho","Nimell.","","kW","3.20","4.20"]
["Huomautukset","","","","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","(2) - Katso toimintalämpötila-alue eri piirustuksesta","(2) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(3) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(3) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(4) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(4) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["Ulkoyksikkö","","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Jäähdytysteho","Nimell.","","kW","","","5.00","5.70"]
["Lämmitysteho","Nimell.","","kW","","","5.80","7.00"]
["Nimellinen tehokkuus","EER","","","","","3.24","3.05"]
["","COP","","","","","3.49","3.41"]
["","Vuotuinen energiankulutus","","kWh","","","771","934"]
["","Energiamerkintädirektiivi","Jäähdytys","","","","A","B"]
["","","Lämmitys","","","","B","B"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","","A+","A+"]
["","Teho","Pdesign","kW","","","5.00","5.70"]
["","SEER","","","","","5.98","5.76"]
["","Vuotuinen energiankulutus","","kWh/a","","","292","347"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","","A","A+"]
["","Teho","Pdesign","kW","","","3.84","3.96"]
["","SCOP/A","","","","","3.90","4.04"]
["","Pdh Lämmitysteho -10°:ssa","","kW","","","3.51","3.66"]
["","Vuotuinen energiankulutus","","kWh/a","","","1377","1372"]