{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXS25L3V1B","FFA35A2VEB / RXS35L3V1B"]
["Jäähdytysteho","Nimell.","","kW","2.50","3.40"]
["Tilan jäähdytys","SEER","","","6.11","6.32"]
["","Vuotuinen energiankulutus","","kWh/a","143","188"]
["","Teho","Pdesign","kW","2.50","3.40"]
["","Energiatehokkuusluokka","","","A++","A++"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Energiatehokkuusluokka","","","A+","A+"]
["","Vuotuinen energiankulutus","","kWh/a","763","1,059"]
["Putkiliitännät","Neste","Ulkohalkaisija","mm","6.35","6.35"]
["","Kaasu","Ulkohalkaisija","mm","9.50","9.50"]
["","Drain","OD","mm","VP20 (ulkohalk. 26, Sisähalk. 20)","VP20 (ulkohalk. 26, Sisähalk. 20)"]
["Nimellinen tehokkuus","EER","","","4.53","3.78"]
["","Vuotuinen energiankulutus","","kWh","276","450"]
["","COP","","","3.90","3.50"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","A","A"]
["Lämmitysteho","Nimell.","","kW","3.20","4.20"]
["Huomautukset","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista","(4) - Katso sähköiset tiedot eri piirustuksista"]