{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / RZASG71M2V1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7V1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7V1B"]
["Jäähdytysteho","Nimell.","","kW","6.80 (1)"]
["Tilan jäähdytys","SEER","","","6.12"]
["","Vuotuinen energiankulutus","","kWh/a","389"]
["","Teho","Pdesign","kW","6.80"]
["","Energiatehokkuusluokka","","","A++"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","4.50"]
["","SCOP/A","","","3.84"]
["","Energiatehokkuusluokka","","","A"]
["","Vuotuinen energiankulutus","","kWh/a","1,641"]
["Lämmitysteho","Nimell.","","kW","7.50 (2)"]
["Huomautukset","","","","(1) - Jäähdytys: T2: sisälämpötila 26,6°CDB, 19,4°CWB, ulkolämpötila 48°CDB [Btu/hr/W]","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["Outdoor unit","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Jäähdytysteho","Nimell.","","kW","","9.50","9.50"]
["Lämmitysteho","Nimell.","","kW","","10.8","10.8"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","A++","A"]
["","Teho","Pdesign","kW","","9.50","9.50"]
["","SEER","","","","6.24","5.49"]
["","Vuotuinen energiankulutus","","kWh/a","","533","606"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","A","A"]
["","Teho","Pdesign","kW","","6.00","6.00"]
["","SCOP/A","","","","3.82","3.90"]
["","Vuotuinen energiankulutus","","kWh/a","","2199","2154"]