{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50N2V1B","FFA60A2VEB9 / RXM60N2V1B"]
["Jäähdytysteho","Nimell.","","kW","5.00"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","772"]
["","EER","","","3.24"]
["","COP","","","3.49"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Lämmitysteho","Nimell.","","kW","5.80"]
["Huomautukset","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista"]
["Outdoor unit","","","","","RXM60N2V1B"]
["Jäähdytysteho","Nimell.","","kW","","5.70"]
["Lämmitysteho","Nimell.","","kW","","7.00"]
["Nimellinen tehokkuus","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Vuotuinen energiankulutus","","kWh","","934"]
["","Energiamerkintädirektiivi","Jäähdytys","","","B"]
["","","Lämmitys","","","B"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","A+"]
["","Teho","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Vuotuinen energiankulutus","","kWh/a","","347"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","A+"]
["","Teho","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Pdh Lämmitysteho -10°:ssa","","kW","","3.66"]
["","Vuotuinen energiankulutus","","kWh/a","","1372"]
["Energiatehokkuusalue","","","","","A+++ ~ D"]