{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B"]
["Energiatehokkuusalue","","","","A+++ ~ D","A+++ ~ D"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","","A","A"]
["","Teho","Pdesign","kW","","","6.80","9.50"]
["","SEER","","","","","5.10","5.10"]
["","Vuotuinen energiankulutus","","kWh/a","","","467","652"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","","A","A"]
["","Teho","Pdesign","kW","","","6.00","11.30"]
["","SCOP/A","","","","","3.80","3.80"]
["","Vuotuinen energiankulutus","","kWh/a","","","2,211","4,164"]