{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Äänenpaineen taso","Lämmitys","Suuri","dBA","36","37","37","38"]
["","","Nimell.","dBA","34","35","35","36"]
["","","Keski","dBA","31","32","33","34"]
["","Jäähdytys","Keski","dBA","34","35","35","36"]
["","","Pieni","dBA","31","32","33","34"]
["","","Suuri","dBA","36","37","37","38"]
["Vakiovarusteet","Lämpöeristeputki","","","2","2","2","2"]
["","Johtimen kiinnitysmateriaali","","","7","7","7","7"]
["","Letkun nauha","","","1","1","1","1"]
["","Tyhjennysletku","","","1","1","1","1"]
["","Aluslevy","","","8","8","8","8"]
["","Tiivistysläppä (suuri)","","","1","1","1","1"]
["","Tiivistysläppä (pieni)","","","1","1","1","1"]
["","Hartsiholkki","","","1","1","1","1"]
["","Ruuvit","","","2","2","2","2"]
["","Johdotuskiinnitin","","","2","2","2","2"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Putkiliitännät","Neste","Ulkohalkaisija","mm","6.35","6.35","6.35","9.52"]
["","Kaasu","Ulkohalkaisija","mm","9.50","12.7","12.7","15.9"]
["","Tyhjennys","","","VP20","VP20","VP20","VP20"]
["Sound power level","Jäähdytys","","dBA","53","54","54","55"]
["Mitat","Yksikkö","Leveys","mm","960","960","1,270","1,270"]
["","","Syvyys","mm","690","690","690","690"]
["","","Korkeus","mm","235","235","235","235"]
["Kotelo","Materiaali","","","Hartsi, teräslevy","Hartsi, teräslevy","Hartsi, teräslevy","Hartsi, teräslevy"]
["","Väri","","","Valkoinen","Valkoinen","Valkoinen","Valkoinen"]
["Paino","Unit","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Vaihe","","","1~","1~","1~","1~"]
["","Taajuus","","Hz","50","50","50","50"]
["","Jännite","","V","220-240","220-240","220-240","220-240"]
["Huomautukset","","","","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista","(1) - Katso sähköiset tiedot eri piirustuksista"]