{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":16,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Tilan jäähdytys","SEER","","","6.95","5.10","5.10","5.10","6.86","6.11","5.10","5.10","5.10","5.10","6.01"]
["","Vuotuinen energiankulutus","","kWh/a","343","467","467","467","347","545","824","652","652","652","699"]
["","Teho","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","12.00","9.50","9.50","9.50","12.00"]
["","Energiatehokkuusluokka","","","A++","B","B","B","A++","A++","B","B","B","B","A+"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","7.60","6.00","6.00","6.00","7.60","11.30","12.71","11.30","11.30","11.30","14.13"]
["","SCOP/A","","","4.32","3.80","3.80","3.80","4.32","4.61","3.80","3.80","3.80","3.80","4.23"]
["","Energiatehokkuusluokka","","","A+","A","A","A","A+","A++","A","A","A","A","A+"]
["","Vuotuinen energiankulutus","","kWh/a","2,463","2,211","2,211","2,211","2,463","3,432","4,683","4,164","4,164","4,164","4,677"]
["Jäähdytysteho","Nimell.","","kW","","","","","6.8","","","","","","","13.4"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","","","","","890","","","","","","","2,025"]
["","EER","","","","","","","3.82","","","","","","","3.31"]
["","COP","","","","","","","4.13","","","","","","","3.63"]
["","Energiamerkintädirektiivi","Jäähdytys","","","","","","A","","","","","","","A"]
["","","Lämmitys","","","","","","A","","","","","","","A"]
["Lämmitysteho","Nimell.","","kW","","","","","7.5","","","","","","","15.5"]
["Huomautukset","","","","","","","","(1) - Vuotuinen energiankulutus ilmoitettu energiamerkintää koskevan direktiivin 2002/31/EY mukaisesti","","","","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","","","","","(2) - SEER ja SCOP ovat EN 14825:n mukaiset","","","","","","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]