{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","33.0","33.0","36.0","36.0"]
["","","","Nimell.","dBA","31.0","31.0","33.0","33.0"]
["","","","Pieni","dBA","28.0","28.0","30.0","30.0"]
["","Jäähdytys","","Keski","dBA","31.0","31.0","33.0","33.0"]
["","","","Pieni","dBA","28.0","28.0","30.0","30.0"]
["","","","Suuri","dBA","33.0","33.0","36.0","36.0"]
["Control systems","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.52","9.52","12.7","12.7"]
["","Kondenssi","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Äänen tehotaso","Jäähdytys","","","dBA","53.0","53.0","56.0","56.0"]
["Mitat","Yksikkö","","Leveys","mm","790","790","1,190","1,190"]
["","","","Syvyys","mm","200","200","200","200"]
["","","","Korkeus","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Kotelo","Materiaali","","","","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy","Galvanoitu teräslevy"]
["","Colour","","","","Maalaamaton","Maalaamaton","Maalaamaton","Maalaamaton"]
["Paino","Yksikkö","","","kg","23.0","23.0","30.0","30.0"]
["Puhallin","Ulkoinen staattinen paine","","Suuri","Pa","48","48","49","49"]
["","","","Nim.","Pa","30","30","40","40"]
["","Ilmamäärä","Lämmitys","Suuri","m³/min","8.7","8.7","16.0","16.0"]
["","","","Pieni","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nimell.","m³/min","8.0","8.0","14.8","14.8"]
["","","Jäähdytys","Pieni","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nimell.","m³/min","8.0","8.0","14.8","14.8"]
["","","","Suuri","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Nimi","","","","VE","VE","VE","VE"]
["","Taajuus","","","Hz","50/60","50/60","50/60","50/60"]
["","Jännite","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Huomautukset","","","","","(1) - Sisältää asennusjalat","(1) - Sisältää asennusjalat","(1) - Sisältää asennusjalat","(1) - Sisältää asennusjalat"]
["","","","","","(2) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(2) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(2) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon.","(2) - Äänitehotaso on absoluuttinen arvo, joka ilmaisee äänilähteen synnyttämän tehon."]