{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","39","40","41","","46"]
["","","","Keski","dBA","32","33","33","","42"]
["","","","Hiljainen toiminta","dBA","19","19","19","","24"]
["","","","Pieni","dBA","25","25","25","","33"]
["","Jäähdytys","","Medium","dBA","32","33","33","","39"]
["","","","Hiljainen toiminta","dBA","19","19","19","","24"]
["","","","Pieni","dBA","25","25","25","","31"]
["","","","Suuri","dBA","39","40","41","","46"]
["Vakiovarusteet","Asennusohje","","","","1","1","1","","1"]
["","Käyttöopas","","","","1","1","1","","1"]
["","Ilmansuodatin","","","","2","2","2","","2"]
["","Infrapunakauko-ohjain","","","","1","1","1","","1"]
["","Kaukosäätimen kiinnityslevy","","","","1","1","1","","1"]
["","Ruuvipussi","","","","1","1","1","","1"]
["","Ruuvinsuoja","","","","1","1","1","","1"]
["","AAA-kuivaparistot","","","","2","2","2","","2"]
["","Yleiset varotoimet","","","","1","1","1","","1"]
["Kylmäaine","GWP","","","","675.0","675.0","675.0","","675.0"]
["Control systems","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Putkistoliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50","9.50","9.50","","12.70"]
["","Tyhjennys","","","","18","18","18","","18"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.020","0.022","0.023","","0.030"]
["","Lämmitys","","Nimell.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Jäähdytys","","","dBA","57","57","60","","60"]
["Mitat","Yksikkö","","Leveys","mm","798","798","798","","798"]
["","","","Syvyys","mm","189","189","189","","189"]
["","","","Korkeus","mm","295","295","295","","295"]
["Kotelo","Colour","","","","Valkoinen","Valkoinen","Valkoinen","","Valkoinen"]
["Paino","Yksikkö","","","kg","11.50","11.50","11.50","","11.50"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Medium","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Pieni","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Hiljainen toiminta","m³/min","4.5","4.5","4.5","","5.7"]
["","","Jäähdytys","Pieni","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Medium","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Suuri","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Hiljainen toiminta","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Vaihe","","","","1~","1~","1~","","1~"]
["","Nimi","","","","V1","V1","V1","","V1"]
["","Taajuus","","","Hz","50","50","50","","50"]
["","Jännite","","","V","220-240","220-240","220-240","","220-240"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","","","0.028"]
["","Lämmitys","","Nimell.","kW","","","","0.036"]
["Kotelo","Väri","","","","","","","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","","","","295"]
["","","","Leveys","mm","","","","798"]
["","","","Syvyys","mm","","","","189"]
["Paino","Yksikkö","","","kg","","","","11.50"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","","","","13.1"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","","","9.8"]
["","","","Pieni","m³/min","","","","7.2"]
["","","","Hiljainen toiminta","m³/min","","","","4.6"]
["","","Lämmitys","Suuri","m³/min","","","","14.6"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","","","","10.5"]
["","","Lämmitys","Pieni","m³/min","","","","7.7"]
["","","","Hiljainen toiminta","m³/min","","","","5.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","","","","60"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","","","","45"]
["","","","Keski","dBA","","","","37"]
["","","","Pieni","dBA","","","","29"]
["","","","Hiljainen toiminta","dBA","","","","21"]
["","Lämmitys","","Suuri","dBA","","","","45"]
["","","","Keski","dBA","","","","37"]
["","","","Pieni","dBA","","","","29"]
["","","","Hiljainen toiminta","dBA","","","","21"]
["Kylmäaine","GWP","","","","","","","675.0"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","","","12.70"]
["","Kondenssi","","","","","","","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","","","","ARC466A58"]
["","Langallinen kaukosäädin","","","","","","","BRC073"]
["Vakiovarusteet","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Ilmansuodatin","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Virransyöttö","Nimi","","","","","","","V1"]
["","Vaihe","","","","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","","","50"]
["","Jännite","","","V","","","","220-240"]