{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-DC / RXA-B8"]
[]
[]
[]
[]
["","","","","FTXA42D2V1BC / RXA42B5V1B8"]
["Jäähdytysteho","Min.","","kW","1.70"]
["","Nimell.","","kW","4.20"]
["","Maks.","","kW","5.00"]
["Lämmitysteho","Min.","","kW","1.70"]
["","Nimell.","","kW","5.40"]
["","Maks.","","kW","6.00"]
["Nimellinen tehokkuus","EER","","","3.99"]
["","COP","","","4.12"]
["","Vuotuinen energiankulutus","","kWh","526"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","4.20"]
["","SEER","","","7.50"]
["","Vuotuinen energiankulutus","","kWh/a","196"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","3.80"]
["","SCOP/A","","","4.60"]
["","Pdh Lämmitysteho -10°:ssa","","kW","3.04"]
["","Vuotuinen energiankulutus","","kWh/a","1156"]
["Energiatehokkuusalue","","","","A+++ ~ D"]
["Huomautukset","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]