{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-C"]
[]
[]
[]
[]
["","","","","","FTXF20C5V1B","FTXF25C5V1B","FTXF35C5V1B","FTXF42C5V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.023","0.023","0.029","0.04"]
["","Lämmitys","","Nimell.","kW","0.023","0.023","0.029","0.04"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","286","286","286","286"]
["","","","Leveys","mm","770","770","770","770"]
["","","","Syvyys","mm","225","225","225","225"]
["Paino","Yksikkö","","","kg","8","8","8.5","9"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","8.3","8.5","11.8","12.6"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","6","6","8","9"]
["","","","Pieni","m³/min","4.6","4.6","6.4","6.9"]
["","","","Hiljainen toiminta","m³/min","3.6","3.6","4.4","4.9"]
["","","Lämmitys","Suuri","m³/min","9.7","9.7","11.9","12.8"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","7.8","7.9","8.6","8.8"]
["","","Lämmitys","Pieni","m³/min","5.8","6","6.5","6.7"]
["","","","Hiljainen toiminta","m³/min","4.6","4.6","5.3","5.2"]
["Äänen tehotaso","Jäähdytys","","","dBA","53","54","54","59"]
["","Lämmitys","","","dBA","55","55","56","59"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39","40","43","45"]
["","","","Keski","dBA","33","33","34","36"]
["","","","Pieni","dBA","25","26","27","30"]
["","","","Hiljainen toiminta","dBA","20","20","20","22"]
["","Lämmitys","","Suuri","dBA","39","40","40","44"]
["","","","Keski","dBA","34","34","35","34"]
["","","","Pieni","dBA","28","28","29","28"]
["","","","Hiljainen toiminta","dBA","21","21","21","22"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5","9.5","9.5"]
["","Kondenssi","","","","18","18","18","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","Langallinen kaukosäädin","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50","50"]
["","Jännite","","","V","220-440","220-440","220-440","220-440"]