{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Jäähdytysteho","Min.","","kW","1.3","1.4"]
["","Maks.","","kW","4.0","4.6"]
["","Nimell.","","kW","2.5 (2)","3.5 (2)"]
["Piping connections","Liquid","Ulkohalkaisija","mm","6.35","6.35"]
["","Gas","Ulkohalkaisija","mm","9.5","9.5"]
["","Tyhjennys","OD","mm","18","18"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","340","490"]
["","EER","","","3.68 (1)","3.57 (1)"]
["","COP","","","4.31 (1)","3.89 (1)"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","A","A"]
["Lämmitysteho","Nimell.","","kW","4.4 (2)","5.1 (2)"]
["","Min.","","kW","1.0 (6)","1.0 (6)"]
["","Maks.","","kW","6.1, 3.6 (7)","6.7, 4.2 (7)"]
["Huomautukset","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]
["","","","","(3) - 220 V","(3) - 220 V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240 V","(5) - 240 V"]
["","","","","(6) - Pienintä nimellistä lämmitystehoa varten aseta sisäyksikön puhallin SL-asentoon","(6) - Pienintä nimellistä lämmitystehoa varten aseta sisäyksikön puhallin SL-asentoon"]
["","","","","(7) - Suurin lämmitysteho -15 °C ulkolämpötilassa","(7) - Suurin lämmitysteho -15 °C ulkolämpötilassa"]