{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Jäähdytysteho","Nimell.","","kW","4.00","","5.20","4.00","6.00","4.00"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","467","","593","471","787","457"]
["","EER","","","4.28","","4.38","4.25","3.81","4.38"]
["","COP","","","4.32","","4.42","4.05","3.88","4.04"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","","A","A","A","A"]
["","","Lämmitys","","A","","A","A","A","A"]
["Lämmitysteho","Nimell.","","kW","4.60","","6.80","6.80","7.80","6.50"]
["Jäähdytysteho","Nimell.","","kW","","4.00"]
["Lämmitysteho","Nimell.","","kW","","4.60"]
["Nimellinen tehokkuus","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Vuotuinen energiankulutus","","kWh","","482"]
["","Energiamerkintädirektiivi","Jäähdytys","","","A"]
["","","Lämmitys","","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","A++"]
["","Teho","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Vuotuinen energiankulutus","","kWh/a","","164"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","A+"]
["","Teho","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh Lämmitysteho -10°:ssa","","kW","","3.58"]
["","Vuotuinen energiankulutus","","kWh/a","","1632"]
["Huomautukset","","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0m."]
["","","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(4) - Katso sähköiset tiedot eri piirustuksista"]