{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["","Lämmitys","","Nimell.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","283","283"]
["","","","Leveys","mm","770","770"]
["","","","Syvyys","mm","198","198"]
["Paino","Yksikkö","","","kg","8.00","8.00"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.3","9.3"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7.7","7.7"]
["","","","Pieni","m³/min","6.1","6.1"]
["","","","Hiljainen toiminta","m³/min","4.9","4.9"]
["","","Lämmitys","Suuri","m³/min","10.1","10.1"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.4","8.4"]
["","","Lämmitys","Pieni","m³/min","6.7","6.7"]
["","","","Hiljainen toiminta","m³/min","5.7","5.7"]
["Äänen tehotaso","Jäähdytys","","","dBA","57","57"]
["","Lämmitys","","","dBA","57","57"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","41","41"]
["","","","Keski","dBA","34","34"]
["","","","Pieni","dBA","27","27"]
["","","","Hiljainen toiminta","dBA","23","23"]
["","Lämmitys","","Suuri","dBA","41","41"]
["","","","Keski","dBA","35","35"]
["","","","Pieni","dBA","29","29"]
["","","","Hiljainen toiminta","dBA","26","26"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50","9.50"]
["","Kondenssi","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Batteries","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Virransyöttö","Nimi","","","","V1","V1"]
["","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]
["Huomautukset","","","","","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V"]