{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 4MWXM-A9"]
[]
[]
[]
[]
["","","","","FTXM25R2V1B / FTXM25R2V1B / 4MWXM52A2V1B9","FTXM25R5V1B / FTXM25R5V1B / 4MWXM52A2V1B9"]
["Jäähdytysteho","Nimell.","","kW","5","5"]
["Lämmitysteho","Nimell.","","kW","6.8","6.8"]
["Nimellinen tehokkuus","EER","","","4.85","4.85"]
["","COP","","","4.45","4.45"]
["","Vuotuinen energiankulutus","","kWh","515","515"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","A","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A+++","A+++"]
["","Teho","Pdesign","kW","5","5"]
["","SEER","","","8.59","8.59"]
["","Vuotuinen energiankulutus","","kWh/a","204","204"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+","A+"]
["","Teho","Pdesign","kW","4.8","4.8"]
["","SCOP/A","","","4.38","4.38"]
["","Pdh Lämmitysteho -10°:ssa","","kW","3.82","3.82"]
["","Vuotuinen energiankulutus","","kWh/a","1533","1533"]
["Huomautukset","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista","(4) - Katso sähköiset tiedot eri piirustuksista"]