{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Jäähdytysteho","Nimell.","","kW","4.00"]
["Lämmitysteho","Nimell.","","kW","4.20"]
["Nimellinen tehokkuus","EER","","","3.71"]
["","COP","","","3.75"]
["","Vuotuinen energiankulutus","","kWh","539"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","4.00"]
["","SEER","","","7.74"]
["","Vuotuinen energiankulutus","","kWh/a","181"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","3.20"]
["","SCOP/A","","","4.30"]
["","Pdh Lämmitysteho -10°:ssa","","kW","2.46"]
["","Vuotuinen energiankulutus","","kWh/a","1041"]
["Energiatehokkuusalue","","","","A+++ ~ D"]
["Huomautukset","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","(4) - Katso sähköiset tiedot eri piirustuksista","(4) - Katso sähköiset tiedot eri piirustuksista"]
["Jäähdytysteho","Nimell.","","kW","","4.00"]
["Lämmitysteho","Nimell.","","kW","","5.20"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","","554"]
["","COP","","","","3.68"]
["","EER","","","","3.61"]
["","Energiamerkintädirektiivi","Jäähdytys","","","A"]
["","","Lämmitys","","","A"]