{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW / RXTA-B"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW / RXTA30B2V1B"]
["Jäähdytysteho","Min.","","kW","0.70"]
["","Nimell.","","kW","3.00"]
["","Maks.","","kW","4.50"]
["Lämmitysteho","Min.","","kW","0.80"]
["","Nimell.","","kW","3.20"]
["","Maks.","","kW","6.90"]
["Nimellinen tehokkuus","EER","","","4.20"]
["","COP","","","4.87"]
["","Vuotuinen energiankulutus","","kWh","357"]
["","Energiamerkintädirektiivi","Jäähdytys","","A"]
["","","Lämmitys","","A"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A++"]
["","Teho","Pdesign","kW","3.00"]
["","SEER","","","7.63"]
["","Vuotuinen energiankulutus","","kWh/a","138"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+++"]
["","Teho","Pdesign","kW","2.60"]
["","SCOP/A","","","5.10"]
["","Pdh Lämmitysteho -10°:ssa","","kW","2.60"]
["","Vuotuinen energiankulutus","","kWh/a","714"]
["Energiatehokkuusalue","","","","A+++ ~ D"]