{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","41"]
["","","","Keski","dBA","31"]
["","","","Hiljainen toiminta","dBA","19"]
["","","","Pieni","dBA","24"]
["","Jäähdytys","","Medium","dBA","32"]
["","","","Hiljainen toiminta","dBA","20"]
["","","","Pieni","dBA","25"]
["","","","Suuri","dBA","43"]
["Vakiovarusteet","Asennusohje","","","","1"]
["","Käyttöopas","","","","1"]
["","Ilmansuodatin","","","","2"]
["","Infrapunakauko-ohjain","","","","1"]
["","Kaukosäätimen kiinnityslevy","","","","1"]
["","Ruuvipussi","","","","1"]
["","Ruuvinsuoja","","","","2"]
["","AAA-kuivaparistot","","","","2"]
["","Yleiset varotoimet","","","","1"]
["Kylmäaine","GWP","","","","675.0"]
["Ohjausjärjestelmät","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Putkistoliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Tyhjennys","","","","18"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.023"]
["","Lämmitys","","Nimell.","kW","0.022"]
["Äänen tehotaso","Jäähdytys","","","dBA","60"]
["","Lämmitys","","","dBA","60"]
["Mitat","Yksikkö","","Leveys","mm","798"]
["","","","Syvyys","mm","189"]
["","","","Korkeus","mm","295"]
["Casing","Colour","","","","Valkoinen"]
["Paino","Yksikkö","","","kg","11.5"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","11.5"]
["","","","Pieni","m³/min","6.0"]
["","","","Keski","m³/min","8.0"]
["","","","Hiljainen toiminta","m³/min","5.1"]
["","","Jäähdytys","Pieni","m³/min","5.7"]
["","","","Keski","m³/min","8.3"]
["","","","Suuri","m³/min","11.9"]
["","","","Hiljainen toiminta","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Taajuus","","","Hz","50"]
["","Nimi","","","","V1"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19.0°CWB; ulkolämpötila 35°CDB, 24°CWB; putkiston ekvivalenttipituus: 5m"]
["","","","","","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista"]