{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-DY"]
[]
[]
[]
[]
["","","","","","FTXTA30D2V1BY"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.023"]
["","Lämmitys","","Nimell.","kW","0.022"]
["Kotelo","Väri","","","","Casing: Black, Panel: Dark wood"]
["Mitat","Yksikkö","","Korkeus","mm","295"]
["","","","Leveys","mm","798"]
["","","","Syvyys","mm","189"]
["Paino","Yksikkö","","","kg","12"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","13.1"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","9.0"]
["","","","Pieni","m³/min","6.0"]
["","","","Hiljainen toiminta","m³/min","4.9"]
["","","Lämmitys","Suuri","m³/min","12.3"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.2"]
["","","Lämmitys","Pieni","m³/min","5.8"]
["","","","Hiljainen toiminta","m³/min","5.0"]
["Äänen tehotaso","Jäähdytys","","","dBA","60"]
["","Lämmitys","","","dBA","60"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","43"]
["","","","Keski","dBA","32"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","20"]
["","Lämmitys","","Suuri","dBA","41"]
["","","","Keski","dBA","31"]
["","","","Pieni","dBA","24"]
["","","","Hiljainen toiminta","dBA","19"]
["Kylmäaine","GWP","","","","675.0"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Kondenssi","","","","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC466A95"]
["","Langallinen kaukosäädin","","","","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Energiatehokkuusalue","","","","","A+++ ~ D"]
["Virransyöttö","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19°CWB, ulkolämpötila 35°CDB, 24°CWB; putkiston ekvivalenttipituus: 5m"]
["","","","","","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista"]