{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.032","0.037"]
["","Lämmitys","","Nimell.","kW","0.037","0.04"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","294","300"]
["","","","Leveys","mm","811","1040"]
["","","","Syvyys","mm","272","295"]
["Paino","Yksikkö","","","kg","10","14.5"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","11.7","15.5"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","8","9.2"]
["","","","Pieni","m³/min","6.3","5.7"]
["","","","Hiljainen toiminta","m³/min","5.2","4.6"]
["","","Lämmitys","Suuri","m³/min","12.2","17.7"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","7.5","11"]
["","","Lämmitys","Pieni","m³/min","5.1","7.5"]
["","","","Hiljainen toiminta","m³/min","4.1","6.3"]
["Äänen tehotaso","Jäähdytys","","","dBA","60","60"]
["","Lämmitys","","","dBA","61","61"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","45","46"]
["","","","Keski","dBA","33","32"]
["","","","Pieni","dBA","25","24"]
["","","","Hiljainen toiminta","dBA","21","20"]
["","Lämmitys","","Suuri","dBA","45","46"]
["","","","Keski","dBA","31","31"]
["","","","Pieni","dBA","22","22"]
["","","","Hiljainen toiminta","dBA","19","19"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5"]
["","Kondenssi","","","","16 (liitäntäletkun sisähalkaisija)","16 (liitäntäletkun sisähalkaisija)"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC466A55","ARC466A55"]
["","Langallinen kaukosäädin","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Virransyöttö","Nimi","","","","V1","V1"]
["","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]