{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","45.0"]
["","","","Keski","dBA","31.0"]
["","","","Hiljainen toiminta","dBA","19.0"]
["","","","Pieni","dBA","22.0"]
["","Jäähdytys","","Keski","dBA","33.0"]
["","","","Hiljainen toiminta","dBA","21.0"]
["","","","Pieni","dBA","25.0"]
["","","","Suuri","dBA","45.0"]
["Vakiovarusteet","Asennusohje","","","","1"]
["","Käyttöopas","","","","1"]
["","Langaton kaukosäädin","","","","1"]
["","AAA-kuivaparistot","","","","2"]
["","Kaukosäätimen pidike","","","","1"]
["","Kiinnityslevy","","","","1"]
["","Sisäyksikön kiinnitysruuvit","","","","2"]
["","Hopeahiukkassuodatin","","","","1"]
["Ohjausjärjestelmät","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Piping connections","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Tyhjennys","","","","18"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.035"]
["","Lämmitys","","Nimell.","kW","0.039"]
["Äänen tehotaso","Jäähdytys","","","dBA","60.0"]
["","Lämmitys","","","dBA","61.0"]
["Mitat","Yksikkö","","Leveys","mm","778"]
["","","","Syvyys","mm","272"]
["","","","Korkeus","mm","295"]
["Kotelo","Colour","","","","Valkoinen"]
["Paino","Yksikkö","","","kg","10.0"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","12.5"]
["","","","Pieni","m³/min","4.9"]
["","","","Medium","m³/min","7.5"]
["","","","Hiljainen toiminta","m³/min","4.0"]
["","","Jäähdytys","Pieni","m³/min","5.3"]
["","","","Medium","m³/min","7.8"]
["","","","Suuri","m³/min","12.2"]
["","","","Hiljainen toiminta","m³/min","4.1"]
["Power supply","Phase","","","","1~"]
["","Taajuus","","","Hz","50"]
["","Nimi","","","","V1"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Jäähdytys: sisälämpötila 27°CDB, 19.0°CWB; ulkolämpötila 35°CDB, 24°CWB; putkiston ekvivalenttipituus: 5m"]
["","","","","","(2) - Lämmitys: sisälämpötila 20°CDB; ulkolämpötila 7°CDB, 6°CWB, kylmäaineputkiston ekvivalenttipituus: 5m"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","0.053"]
["","Lämmitys","","Nimell.","kW","","0.06"]
["Kotelo","Väri","","","","","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","","299"]
["","","","Leveys","mm","","998"]
["","","","Syvyys","mm","","292"]
["Paino","Yksikkö","","","kg","","14.5"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","","15.4"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","9.5"]
["","","","Pieni","m³/min","","5.8"]
["","","","Hiljainen toiminta","m³/min","","4.6"]
["","","Lämmitys","Suuri","m³/min","","17.5"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","","10.5"]
["","","Lämmitys","Pieni","m³/min","","7.1"]
["","","","Hiljainen toiminta","m³/min","","5.9"]
["Äänen tehotaso","Jäähdytys","","","dBA","","60"]
["","Lämmitys","","","dBA","","61"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","","46"]
["","","","Keski","dBA","","32"]
["","","","Pieni","dBA","","24"]
["","","","Hiljainen toiminta","dBA","","20"]
["","Lämmitys","","Suuri","dBA","","46"]
["","","","Keski","dBA","","31"]
["","","","Pieni","dBA","","22"]
["","","","Hiljainen toiminta","dBA","","19"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","9.5"]
["","Kondenssi","","","","","18"]
["Ohjausjärjestelmät","Infrared remote control","","","","","ARC466A75"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Virransyöttö","Nimi","","","","","V1"]
["","Vaihe","","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]