{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.035","0.053"]
["","Lämmitys","","Nimell.","kW","0.039","0.06"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","295","299"]
["","","","Leveys","mm","778","998"]
["","","","Syvyys","mm","272","292"]
["Paino","Yksikkö","","","kg","10","15"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","11.5","15.1"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7.5","9.2"]
["","","","Pieni","m³/min","5.2","5.6"]
["","","","Hiljainen toiminta","m³/min","4.2","4.8"]
["","","Lämmitys","Suuri","m³/min","11.6","17"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","7.3","10"]
["","","Lämmitys","Pieni","m³/min","4.7","6"]
["","","","Hiljainen toiminta","m³/min","4","5.1"]
["Äänen tehotaso","Jäähdytys","","","dBA","60","60"]
["","Lämmitys","","","dBA","60","60"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","45","46"]
["","","","Keski","dBA","33","32"]
["","","","Pieni","dBA","25","24"]
["","","","Hiljainen toiminta","dBA","21","20"]
["","Lämmitys","","Suuri","dBA","45","46"]
["","","","Keski","dBA","31","31"]
["","","","Pieni","dBA","22","22"]
["","","","Hiljainen toiminta","dBA","19","19"]
["Kylmäaine","GWP","","","","675","675"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5"]
["","Kondenssi","","","","18","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC466A83","ARC466A83"]
["","Langallinen kaukosäädin","","","","BRC073A1","BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]