{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","43"]
["","","","Keski","dBA","35"]
["","","","Hiljainen toiminta","dBA","21"]
["","","","Pieni","dBA","26"]
["","Jäähdytys","","Keski","dBA","35"]
["","","","Hiljainen toiminta","dBA","21"]
["","","","Pieni","dBA","26"]
["","","","Suuri","dBA","43"]
["Vakiovarusteet","Asennusohje","","","","1"]
["","Käyttöopas","","","","1"]
["","Langaton kaukosäädin","","","","1"]
["","AAA-kuivaparistot","","","","2"]
["","Kaukosäätimen pidike","","","","1"]
["","Kiinnityslevy","","","","1"]
["","Raikastava titaani-apatiitti-suodatin","","","","2"]
["","Sisäyksikön kiinnitysruuvit","","","","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Kondenssi","","","","16 (liitäntäletkun sisähalkaisija)"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.030"]
["","Lämmitys","","Nimell.","kW","0.035"]
["Äänen tehotaso","Jäähdytys","","","dBA","58"]
["","Lämmitys","","","dBA","58"]
["Mitat","Yksikkö","","Leveys","mm","770"]
["","","","Syvyys","mm","225"]
["","","","Korkeus","mm","285"]
["Kotelo","Colour","","","","Valkoinen"]
["Paino","Yksikkö","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Taajuus","","","Hz","50"]
["","Nimi","","","","V1"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Katso sähköiset tiedot eri piirustuksista"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","0.03"]
["","Lämmitys","","Nimell.","kW","","0.035"]
["Kotelo","Väri","","","","","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","","285"]
["","","","Leveys","mm","","770"]
["","","","Syvyys","mm","","225"]
["Paino","Yksikkö","","","kg","","9"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","","11.4"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","","8.2"]
["","","","Pieni","m³/min","","5.4"]
["","","","Hiljainen toiminta","m³/min","","4.3"]
["","","Lämmitys","Suuri","m³/min","","10.8"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","","7.8"]
["","","Lämmitys","Pieni","m³/min","","5.8"]
["","","","Hiljainen toiminta","m³/min","","4.9"]
["Äänen tehotaso","Jäähdytys","","","dBA","","58"]
["","Lämmitys","","","dBA","","58"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","","43"]
["","","","Keski","dBA","","35"]
["","","","Pieni","dBA","","26"]
["","","","Hiljainen toiminta","dBA","","21"]
["","Lämmitys","","Suuri","dBA","","43"]
["","","","Keski","dBA","","35"]
["","","","Pieni","dBA","","26"]
["","","","Hiljainen toiminta","dBA","","21"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","9.5"]
["","Kondenssi","","","","","16 (liitäntäletkun sisähalkaisija)"]
["Control systems","Infrared remote control","","","","","ARC480A11"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","","","BRC944B2, BRC073A1"]
["Vakiovarusteet","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Virransyöttö","Nimi","","","","","V1"]
["","Vaihe","","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]