{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","39","42","44"]
["","","","Hiljainen toiminta","dBA","19","19","24"]
["","","","Pieni","dBA","28","29","31"]
["","Jäähdytys","","Hiljainen toiminta","dBA","19","19","23"]
["","","","Pieni","dBA","26","27","30"]
["","","","Suuri","dBA","38","42","47"]
["","","","Nimell.","dBA","35","36","38"]
["","Jäähdytys","","Nimell.","dBA","33","35","38"]
["Vakiovarusteet","Fotokatalyyttinen Ilmanpuhdistussuodatin, jossa on hajunpoistotoiminto","","","","1","1","1"]
["","Langaton kaukosäädin","","","","1","1","1"]
["","Kuivaparistot","","","","2","2","2"]
["","Kaukosäätimen pidike","","","","1","1","1"]
["","Sisäyksikön kiinnitysruuvit","","","","3","3","3"]
["","Kiinnityslevy","","","","1","1","1"]
["Ohjausjärjestelmät","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Piping connections","Neste","","Ulkohalkaisija","mm","6.35","6.35","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5","9.5"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.030","0.030","0.030"]
["","Lämmitys","","Nimell.","kW","0.030","0.030","0.030"]
["Äänen tehotaso","Jäähdytys","","","dBA","54","57","60"]
["","Lämmitys","","","dBA","56","57","59"]
["Mitat","Yksikkö","","Leveys","mm","798","798","798"]
["","","","Syvyys","mm","372","372","372"]
["","","","Korkeus","mm","295","295","295"]
["Kotelo","Colour","","","","Valkoinen","Valkoinen","Valkoinen"]
["Paino","Yksikkö","","","kg","15","15","15"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","11.7","13.3","14.4"]
["","","","Pieni","m³/min","6.7","6.9","7.7"]
["","","","Hiljainen toiminta","m³/min","4.8","4.8","5.9"]
["","","Jäähdytys","Pieni","m³/min","5.3","5.6","6.6"]
["","","","Suuri","m³/min","10.7","12.1","15.0"]
["","","","Hiljainen toiminta","m³/min","4.0","4.0","4.6"]
["","","","Nimell.","m³/min","8.6","9.2","10.7"]
["","","Jäähdytys","Nimell.","m³/min","7.5","8.4","9.2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Nimi","","","","V1","V1","V1"]
["","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]
["Huomautukset","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Lämmönvaihtimen etuosa","(4) - Lämmönvaihtimen etuosa","(4) - Lämmönvaihtimen etuosa"]
["","","","","","(5) - Lämmönvaihtimen takaosa","(5) - Lämmönvaihtimen takaosa","(5) - Lämmönvaihtimen takaosa"]