{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / RZASG100M7V1B","FUA125AVEB9 / RZASG125M7V1B","FUA71AVEB / RZASG71M2V1B","FUA71AVEB9 / RZASG71M2V1B","FUA71AVEB9 / FUA71AVEB9 / RZASG140M7V1B"]
["Jäähdytysteho","Nimell.","","kW","","","6.80 (1)","6.80 (1)"]
["Tilan jäähdytys","SEER","","","","","6.16","6.16"]
["","Vuotuinen energiankulutus","","kWh/a","","","386","386"]
["","Teho","Pdesign","kW","","","6.80","6.80"]
["","Energiatehokkuusluokka","","","","","A++","A++"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","","","4.50","4.50"]
["","SCOP/A","","","","","3.90","3.90"]
["","Energiatehokkuusluokka","","","","","A","A"]
["","Vuotuinen energiankulutus","","kWh/a","","","1,615","1,615"]
["Lämmitysteho","Nimell.","","kW","","","7.50 (2)","7.50 (2)"]
["Huomautukset","","","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","","(4) - Katso sähköiset tiedot eri piirustuksista","(4) - Katso sähköiset tiedot eri piirustuksista"]
["Jäähdytysteho","Nimell.","","kW","9.5","12.1","","","13.4"]
["Lämmitysteho","Nimell.","","kW","10.8","13.5","","","15.5"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","9.5","12.1","","","13.4"]
["","SEER","","","5.83","5.49","","","8.56"]
["","Vuotuinen energiankulutus","","kWh/a","570","1322","","","939"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","6","6","","","7.80"]
["","SCOP/A","","","4.01","3.84","","","5.00"]
["","Vuotuinen energiankulutus","","kWh/a","2095","2188","","","2185"]