{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","","","41","46","47"]
["","","","Keski","dBA","","","","38","42","43"]
["","","","Pieni","dBA","","","","35","39","40"]
["","Jäähdytys","","Keski","dBA","","","","38","42","43"]
["","","","Pieni","dBA","","","","35","39","40"]
["","","","Suuri","dBA","","","","41","46","47"]
["Vakiovarusteet","Käyttöopas","","","","","","","1","1","1"]
["","Asennusohje","","","","","","","1","1","1"]
["","Tyhjennysletku","","","","","","","1","1","1"]
["","Lämpöeristeputki","","","","","","","3","3","3"]
["","Nippusiteet","","","","","","","10","10","10"]
["","Letkun nauha","","","","","","","1","1","1"]
["","Tiivistysmateriaali","","","","","","","4","4","4"]
["","Kiinnityslevyn aluslevy","","","","","","","1","1","1"]
["","Tyhjennysliitos","","","","","","","1","1","1"]
["","Kuitukangas","","","","","","","1","1","1"]
["","Aluslevy","","","","","","","8","8","8"]
["","Tyhjennysputken kiinnitysruuvi","","","","","","","5","5","5"]
["Ohjausjärjestelmät","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Jäähdytysteho","Yhteisteho","","Nimell.","kW","","","","","","12.1"]
["Piping connections","Neste","","Ulkohalkaisija","mm","","","","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","","","","15.9","15.9","15.9"]
["","Tyhjennys","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Äänen tehotaso","Jäähdytys","","","dBA","","","","59","64","65"]
["","Lämmitys","","","dBA","","","","59","64"]
["Mitat","Yksikkö","","Leveys","mm","","","","950","950","950"]
["","","","Syvyys","mm","","","","950","950","950"]
["","","","Korkeus","mm","","","","198","198","198"]
["Kotelo","Materiaali","","","","","","","Hartsi","Hartsi","Hartsi"]
["","Colour","","","","","","","Raikas valkoinen","Raikas valkoinen","Raikas valkoinen"]
["Paino","Yksikkö","","","kg","","","","25.0","26.0","26"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","","","","23.0","31.0","32.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Pieni","m³/min","","","","16.0","20.0","20.5"]
["","","Jäähdytys","Pieni","m³/min","","","","16.0","20.0","20.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Suuri","m³/min","","","","23.0","31.0","32.5"]
["Nostokorkeus","mm","","","","","","","600","600","600"]
["Lämmitysteho","Yhteisteho","","Nim.","kW","","","","","","13.5"]
["Kotelo","Väri","","","","Raikas valkoinen","Raikas valkoinen","Raikas valkoinen"]
["","Materiaali","","","","Hartsi","Hartsi","Hartsi"]
["Mitat","Yksikkö","","Korkeus","mm","198","198","198"]
["","","","Leveys","mm","950","950","950"]
["","","","Syvyys","mm","950","950","950"]
["Paino","Yksikkö","","","kg","25.0","26.0","26.0"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","23.0","31.0","32.5"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","19.5","25.5","26.5"]
["","","","Pieni","m³/min","16.0","20.0","20.5"]
["","","Lämmitys","Suuri","m³/min","23.0","31.0","32.5"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","19.5","25.5","26.5"]
["","","Lämmitys","Pieni","m³/min","16.0","20.0","20.5"]
["Äänen tehotaso","Jäähdytys","","","dBA","59","64","65"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","41","46","47"]
["","","","Keski","dBA","38","42","43"]
["","","","Pieni","dBA","35","39","40"]
["","Lämmitys","","Suuri","dBA","41","46","47"]
["","","","Keski","dBA","38","42","43"]
["","","","Pieni","dBA","35","39","40"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.9","15.9","15.9"]
["","Kondenssi","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Nostokorkeus","mm","","","","600","600","600"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Jäähdytysteho","Kokonaisteho","","Nimell.","kW","","","12.10"]
["Lämmitysteho","Yhteisteho","","Nim.","kW","","","13.5"]