{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L9V1B","FUQ71CVEB / RZQG71L9V1B","FUQ100CVEB / RZQG100L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG100L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG125L9V1B","FUQ125CVEB / RZQG125L9V1B"]
["Jäähdytysteho","Nimell.","","kW","","6.8","9.5","","","12.0"]
["Tilan jäähdytys","SEER","","","6.50","6.42","6.11","5.10","5.10","5.61"]
["","Vuotuinen energiankulutus","","kWh/a","367","371","545","652","824","749"]
["","Teho","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Energiatehokkuusluokka","","","A++","A++","A++","B","B","A+"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","7.60","7.60","11.30","11.30","12.71","14.13"]
["","SCOP/A","","","4.20","4.20","4.50","3.80","3.80","4.44"]
["","Energiatehokkuusluokka","","","A+","A+","A+","A","A","A+"]
["","Vuotuinen energiankulutus","","kWh/a","2,534","2,534","3,516","4,164","4,683","4,456"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","","840","1,230","","","1,770"]
["","EER","","","","4.05","3.86","","","3.39"]
["","COP","","","","4.08","3.95","","","3.42"]
["","Energiamerkintädirektiivi","Jäähdytys","","","A","A","","","A"]
["","","Lämmitys","","","A","A","","","B"]
["Lämmitysteho","Nimell.","","kW","","7.5","10.8","","","13.5"]
["Huomautukset","","","","","(1) - Vuotuinen energiankulutus ilmoitettu energiamerkintää koskevan direktiivin 2002/31/EY mukaisesti","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","","(2) - SEER ja SCOP ovat EN 14825:n mukaiset","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla","","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]