{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Äänenpaineen taso","Lämmitys","Suuri","dBA","41","46","47"]
["","","Nimell.","dBA","38","42","43"]
["","","Pieni","dBA","35","39","40"]
["","Jäähdytys","Pieni","dBA","35","39","40"]
["","","Suuri","dBA","41","46","47"]
["","","Nimell.","dBA","38","42","43"]
["Vakiovarusteet","Asennusohje","","","Asennusohje","Asennusohje","Asennusohje"]
["","Käyttöopas","","","Käyttöopas","Käyttöopas","Käyttöopas"]
["","Vaatimustenmukaisuusvakuutus","","","Vaatimustenmukaisuusvakuutus","Vaatimustenmukaisuusvakuutus","Vaatimustenmukaisuusvakuutus"]
["","Tyhjennysletku","","","Tyhjennysletku","Tyhjennysletku","Tyhjennysletku"]
["","Metalliside","","","Metalliside","Metalliside","Metalliside"]
["","Koukkukiinnikkeen aluslevy","","","Koukkukiinnikkeen aluslevy","Koukkukiinnikkeen aluslevy","Koukkukiinnikkeen aluslevy"]
["","Siteet","","","Siteet","Siteet","Siteet"]
["","Letkunkiristin","","","Letkunkiristin","Letkunkiristin","Letkunkiristin"]
["","Liitoksen eristys- ja tiivistysmateriaali","","","Liitoksen eristys- ja tiivistysmateriaali","Liitoksen eristys- ja tiivistysmateriaali","Liitoksen eristys- ja tiivistysmateriaali"]
["","Mutka","","","Mutka","Mutka","Mutka"]
["","Asennuskuvio","","","Asennuskuvio","Asennuskuvio","Asennuskuvio"]
["","Suljinmateriaali","","","Suljinmateriaali","Suljinmateriaali","Suljinmateriaali"]
["","L-taivutetut putket","","","L-taivutetut putket","L-taivutetut putket","L-taivutetut putket"]
["","Ruuvit","","","Ruuvit","Ruuvit","Ruuvit"]
["","Kuitukangas","","","Kuitukangas","Kuitukangas","Kuitukangas"]
["Ohjausjärjestelmät","Langallinen kaukosäädin","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Putkiliitännät","Neste","Ulkohalkaisija","mm","9.52","9.52","9.52"]
["","Kaasu","Ulkohalkaisija","mm","15.9","15.9","15.9"]
["","Tyhjennys","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Jäähdytys","","dBA","59","64","65"]
["","Lämmitys","","dBA","59","64","65"]
["Mitat","Yksikkö","Leveys","mm","950","950","950"]
["","","Syvyys","mm","950","950","950"]
["","","Korkeus","mm","198","198","198"]
["Kotelo","Materiaali","","","Hartsi","Hartsi","Hartsi"]
["","Väri","","","Raikas valkoinen","Raikas valkoinen","Raikas valkoinen"]
["Paino","Unit","","kg","25","26","26"]
["Nostokorkeus","mm","","","600","600","600"]
["Power supply","Phase","","","1~","1~","1~"]
["","Taajuus","","Hz","50/60","50/60","50/60"]
["","Nimi","","","VE","VE","VE"]
["","Jännite","","V","220-240/220","220-240/220","220-240/220"]