{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZASG100M7Y1B","FVA125AMVEB / RZASG125M7Y1B","FVA140AMVEB / RZASG140M7Y1B","FVA71AMVEB / FVA71AMVEB / RZASG140M7Y1B"]
["Jäähdytysteho","Nimell.","","kW","","12.1 (1)","13.4 (1)"]
["Space cooling","Vuotuinen energiankulutus","","kWh/a","","1,314","1,428"]
["","Teho","Pdesign","kW","","12.1","13.4"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","","6.00","7.80"]
["","Vuotuinen energiankulutus","","kWh/a","","2,308","2,866"]
["Lämmitysteho","Nimell.","","kW","","13.5 (2)","15.5 (2)"]
["Jäähdytysteho","Nimell.","","kW","9.5","","","13.4"]
["Lämmitysteho","Nimell.","","kW","10.8","","","15.5"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","A+"]
["","Teho","Pdesign","kW","9.5","","","13.4"]
["","SEER","","","5.72","","","7.71"]
["","Vuotuinen energiankulutus","","kWh/a","581","","","1043"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","A"]
["","Teho","Pdesign","kW","6","","","7.80"]
["","SCOP/A","","","3.83","","","4.43"]
["","Vuotuinen energiankulutus","","kWh/a","2193","","","2467"]
["Space cooling","SEER","","","","5.52","5.63"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","SCOP/A","","","","3.64","3.81"]
["Huomautukset","","","","","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","(1) - Nim. jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0m."]
["","","","","","(3) - Katso toimintalämpötila-alue eri piirustuksesta","(3) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(4) - Katso sähköiset tiedot eri piirustuksista","(4) - Katso sähköiset tiedot eri piirustuksista"]
["Energiatehokkuusalue","","","","","","","A+++ ~ D"]